# Myers_Reservoir.tif

## Raster Dataset - TIFF

Description | Spatial | Attributes

Keywords
Theme: DRG, Wyoming
Theme: DRG, 7.5 minute
Description
Abstract

    Digital Raster Graphic of a 7.5 minute quadrangle in 1:24000 scale

Purpose

    This is basic GIS data

Supplementary Information

    This dataset was obtained from Idaho State University's GIS Training and Research Center.

_________________
Status of the data
Complete
Data update frequency: As needed
Time period for which the data is relevant
Date and time: Late 1900's
Description:

    publication date

Publication Information
Who created the data: USGS
Date and time: Various
_________________
Data storage and access information
File name: Myers_Reservoir.tif
Type of data: remote-sensing image
Location of the data:
- http://giscenter-sl.isu.edu/AOC/AOC_DRG/Wyoming/Myers_Reservoir.zip
Data processing environment: Microsoft Windows XP Version 5.1 (Build 2600) Service Pack 2; ESRI ArcCatalog 9.1.0.722
Accessing the data
Size of the data: 0.000 MB
Data transfer size: 0.000 MB
Constraints on accessing and using the data
Access constraints: No constraints have been placed on access of this dataset.
Use constraints:

    This dataset can be used in any fashion deemed acceptable by the end-user.  The GIS Center at ISU advises that users apply the dataset in ways appropriate to its source scale and original intent.  The end-user is responsible to understand the errors, bias, and uncertainty inherit in this and all GIS datasets.

Details about this document
Contents last updated: 20060531 at time 12572700
Contents last reviewed: unk
Contents to be reviewed: unk
Who completed this document
Scott Taylor
ISU's GIS TReC
mailing address:

    Campus Box 8104

Pocatello, Idaho 83209-8104
USA
208 282 3606 (voice)
208 282 5802 (fax)
giscenter@isu.edu
Hours of service: 9am-4pm
Contact Instructions:

    When contacting the GIS Center with questions about the preparation and documentation of this metadata file please use e-mail. Include METADATA QUESTION in the subject line and fully identify the document with which you have a question.

Standards used to create this document
Standard name: FGDC Content Standards for Digital Geospatial Metadata
Standard version: FGDC-STD-001-1998
Time convention used in this document: local time
Metadata profiles defining additonal information
- ESRI Metadata Profile: http://www.esri.com/metadata/esriprof80.html
Horizontal coordinate system
Projected coordinate system name: Transverse Mercator
Geographic coordinate system name: GCS_North_American_1927
Details
Map Projection Name: Transverse Mercator
Scale Factor at Central Meridian: 0.999600
Longitude of Central Meridian: -114.000000
Latitude of Projection Origin: 42.000000
False Easting: 500000.000000
False Northing: 100000.000000
Planar Coordinate Information
Planar Distance Units: meters
Coordinate Encoding Method: row and column
Coordinate Representation
Abscissa Resolution: 2.551679
Ordinate Resolution: 2.551679
Geodetic Model
Horizontal Datum Name: North American Datum of 1927
Ellipsoid Name: Clarke 1866
Semi-major Axis: 6378206.400000
Denominator of Flattening Ratio: 294.978698
_________________
Bounding coordinates
Horizontal
In decimal degrees
West: -111.017680
East: -110.857084
North: 41.137160
South: 40.980139
In projected or local coordinates
Left: 750900.310195
Right: 763816.911712
Top: 8516.320266
Bottom: -8485.520096
_________________
Lineage
FGDC lineage
Process step 1
Process description: Dataset copied.
Source used: C:\Data\GIS\AOCBasic\aocstates
_________________
Spatial data description
Vector data information
ESRI description
aocstates
ESRI feature type: Simple
Geometry type: Polygon
Topology: FALSE
Feature count: 5
Spatial Index: FALSE
Linear referencing: FALSE
SDTS description
Feature class: SDTS feature type, feature count
- aocstates: G-polygon, 5
Raster dataset information
Raster format: TIFF
SDTS raster type: Pixel
Number of raster bands: 1
Raster properties
Origin location: Upper Left
Has pyramids: FALSE
Has colormap: TRUE
Data compression type: PackBits
Display type: pixel codes
Cell information
Number of cells on x-axis: 5062
Number of cells on y-axis: 6663
Number of cells on z-axis: 1
Number of bits per cell: 8
Cell Size
X distance: 2.551679
Y distance: 2.551679
Details for Band_1
Type of object: Table
Number of records: 256
Attributes
ObjectID
Alias: ObjectID
Data type: OID
Width: 4
Precision: 0
Scale: 0
Definition:

    Internal feature number.

Definition Source:

    ESRI

Value
Alias: Value
Data type: Integer
Width: 0
Precision: 0
Scale: 0
Red
Alias: Red
Data type: Double
Width: 0
Precision: 0
Scale: 0
Green
Alias: Green
Data type: Double
Width: 0
Precision: 0
Scale: 0
Blue
Alias: Blue
Data type: Double
Width: 0
Precision: 0
Scale: 0