lasinfo (250415) report for 'output\USGS_LPC_ID_2023BlaineCaribou_C25_814471.laz'
reporting all LAS header entries:
  file signature:             'LASF'
  file source ID:             0
  global_encoding:            17
  project ID GUID data 1-4:   D2EFB29F-9377-4447-81F2-4455977A7E9E
  version major.minor:        1.4
  system identifier:          'LAStools (c) by rapidlasso GmbH'
  generating software:        'lasduplicate64 (250415) academi'
  file creation day/year:     190/2025
  header size:                375
  offset to point data:       1453
  number var. length records: 1
  point data format:          6
  point data record length:   30
  number of point records:    0
  number of points by return: 0 0 0 0 0
  scale factor x y z:         0.01 0.01 0.01
  offset x y z:               800000 400000 0
  min x y z:                  814903.00 471565.00 6726.46
  max x y z:                  817903.00 474564.99 7564.25
  start of waveform data packet record: 0
  start of first extended variable length record: 0
  number of extended_variable length records: 0
  extended number of point records: 19751353
  extended number of points by return: 14049606 3970879 1369392 308179 47691 5209 377 20 0 0 0 0 0 0 0
variable length header record 1 of 1:
  reserved             0
  user ID              'LASF_Projection'
  record ID            2112
  length after header  1024
  description          'WKT Projection'
    WKT OGC COORDINATE SYSTEM:
    COMPD_CS["NAD83(2011) / Idaho East (ftUS) + NAVD88 height (ftUS) - Geoid18 (ftUS)",PROJCS["NAD83(2011) / Idaho East (ftUS)",GEOGCS["NAD83(2011)",DATUM["NAD83 (National Spatial Reference System 2011)",SPHEROID["GRS 1980",6378137,298.257222101,AUTHORITY["EPSG","7019"]],AUTHORITY["EPSG","1116"]],PRIMEM["Greenwich",0,AUTHORITY["EPSG","8901"]],UNIT["degree",0.0174532925199433,AUTHORITY["EPSG","9122"]],AUTHORITY["EPSG","6318"]],PROJECTION["Transverse_Mercator"],PARAMETER["latitude_of_origin",41.66666666666666],PARAMETER["central_meridian",-112.1666666666667],PARAMETER["scale_factor",0.999947368],PARAMETER["false_easting",656166.667],PARAMETER["false_northing",0],UNIT["US survey foot",0.3048006096012192,AUTHORITY["EPSG","9003"]],AXIS["X",EAST],AXIS["Y",NORTH],AUTHORITY["EPSG","6451"]],VERT_CS["NAVD88 height (ftUS) - Geoid18 (ftUS)",VERT_DATUM["North American Vertical Datum 1988",2005,AUTHORITY["EPSG","5103"]],UNIT["US survey foot",0.3048006096012192,AUTHORITY["EPSG","9003"]],AXIS["Up",UP],AUTHORITY["EPSG","6360"]]]
LASzip compression (version 3.4r4 c3 50000): POINT14 3
reporting minimum and maximum for all LAS point record entries ...
  X             1490300    1790300
  Y             7156500    7456499
  Z              672646     756425
  intensity           0      41470
  return_number       1          7
  number_of_returns   1          7
  edge_of_flight_line 0          1
  scan_direction_flag 0          1
  classification      1         18
  scan_angle_rank   -29         30
  user_data           0          0
  point_source_ID   121        124
  gps_time 379557890.843572 379600021.997230
  extended_return_number          1      8
  extended_number_of_returns      1      8
  extended_classification         1     18
  extended_scan_angle         -4880   4928
  extended_scanner_channel        1      2
number of first returns:        14049606
number of intermediate returns: 1717407
number of last returns:         14067858
number of single returns:       10083518
covered area in square meters/kilometers: 8981248/8.98
point density: all returns 2.20 last only 1.57 (per square meter)
      spacing: all returns 0.67 last only 0.80 (in meters)
overview over extended number of returns of given pulse: 10083518 5214711 3175890 1035359 210604 28638 2471 162 0 0 0 0 0 0 0
histogram of classification of points:
        12370007  unclassified (1)
         7376636  ground (2)
            4529  noise (7)
             181  Reserved for ASPRS Definition (18)
 +-> flagged as withheld:  4710
  +--->            4529 of those are noise (7)
  +--->             181 of those are Reserved for ASPRS Definition (18)
