# BEAR_LAKE_SOUTH_UT_SW.sid

## Metadata:

- Identification_Information
- Data_Quality_Information
- Spatial_Data_Organization_Information
- Spatial_Reference_Information
- Entity_and_Attribute_Information
- Distribution_Information
- Metadata_Reference_Information

Identification_Information:
  Citation:
    Citation_Information:
      Originator: U.S. Geological Survey
      Publication_Date: 19920827
      Title:
        BEAR_LAKE_SOUTH_UT_SW.sid
      Geospatial_Data_Presentation_Form: remote-sensing image
      Online_Linkage: http://giscenter-sl.isu.edu/AOC/AOC_DOQQ/Utah/BEAR_LAKE_SOUTH_UT_SW.zip
  Description:
    Abstract:

        This is a DOQQ of a region of Utah.  DOQQs are Digital Orthophoto Quarter Quads - each Quad is split into
        NW, NE, SE, and SW quadrats.  Therefore, to obtain an entire quad
        requires that you download 4 files.  The quarter quad is indicated in
        the download file name.

    Purpose:

        This is basic GIS data.  This dataset can be used in any fashion deemed acceptable by the end-user.

    Supplemental_Information:

        This dataset was obtained from Idaho State University's GIS Training and Research Center.

  Time_Period_of_Content:
    Time_Period_Information:
      Single_Date/Time:
        Calendar_Date: 19920827
    Currentness_Reference:

        publication date

  Status:
    Progress: Complete
    Maintenance_and_Update_Frequency: None planned
  Spatial_Domain:
    Bounding_Coordinates:
      West_Bounding_Coordinate: -111.319299
      East_Bounding_Coordinate: -111.242439
      North_Bounding_Coordinate: 42.004609
      South_Bounding_Coordinate: 41.932962
  Keywords:
    Theme:
      Theme_Keyword_Thesaurus: NA
      Theme_Keyword: imagery
      Theme_Keyword: DOQ
      Theme_Keyword: DOQQ
      Theme_Keyword: digital orthophoto quadrangle data
      Theme_Keyword: digital orthophoto quarter quadrangle data
      Theme_Keyword: 010
  Access_Constraints: No constraints have been placed on access of this dataset.
  Use_Constraints:

      This dataset can be used in any fashion deemed acceptable by the end-user.  The GIS Center at ISU advises that users apply the dataset in ways appropriate to its source scale and original intent.  The end-user is responsible to understand the errors, bias, and uncertainty inherit in this and all GIS datasets.

  Point_of_Contact:
    Contact_Information:
      Contact_Organization_Primary:
        Contact_Organization: ISU GIS TReC
        Contact_Person: Keith T. Weber, GISP
      Contact_Position: GIS Director
      Contact_Address:
        Address_Type: mailing address
        Address:

            Campus Box 8104

        City: Pocatello
        State_or_Province: Idaho
        Postal_Code: 83209-8104
        Country: USA
      Contact_Voice_Telephone: 208 282 3606
      Contact_Facsimile_Telephone: 208 282 5802
      Contact_Electronic_Mail_Address: giscenter@isu.edu
  Data_Set_Credit:

      Made available by Idaho State University's GIS Training and Research Center

  Security_Information:
    Security_Classification_System: none
    Security_Classification: Unclassified
  Native_Data_Set_Environment:
    Microsoft Windows XP Version 5.1 (Build 2600) Service Pack 2; ESRI ArcCatalog 9.1.0.722

Back to Top

Data_Quality_Information:
  Lineage:
    Process_Step:
      Process_Description:

          Dataset copied.

      Source_Used_Citation_Abbreviation:
        C:\Data\GIS\AOCBasic\aocstates

Back to Top

Spatial_Data_Organization_Information:
  Direct_Spatial_Reference_Method: Raster
  Point_and_Vector_Object_Information:
    SDTS_Terms_Description:
      SDTS_Point_and_Vector_Object_Type: G-polygon
      Point_and_Vector_Object_Count: 5
  Raster_Object_Information:
    Raster_Object_Type: Pixel
    Row_Count: 7433
    Column_Count: 5864
    Vertical_Count: 1

Back to Top

Spatial_Reference_Information:
  Horizontal_Coordinate_System_Definition:
    Planar:
      Map_Projection:
        Map_Projection_Name: Transverse Mercator
        Transverse_Mercator:
          Scale_Factor_at_Central_Meridian: 0.999600
          Longitude_of_Central_Meridian: -114.000000
          Latitude_of_Projection_Origin: 42.000000
          False_Easting: 500000.000000
          False_Northing: 100000.000000
      Planar_Coordinate_Information:
        Planar_Coordinate_Encoding_Method: row and column
        Coordinate_Representation:
          Abscissa_Resolution: 1.045197
          Ordinate_Resolution: 1.045197
        Planar_Distance_Units: meters
    Geodetic_Model:
      Horizontal_Datum_Name: North American Datum of 1927
      Ellipsoid_Name: Clarke 1866
      Semi-major_Axis: 6378206.400000
      Denominator_of_Flattening_Ratio: 294.978698

Back to Top

Entity_and_Attribute_Information:
  Detailed_Description:
    Entity_Type:
      Entity_Type_Label: Band_1
    Attribute:
      Attribute_Label: ObjectID
      Attribute_Definition:

          Internal feature number.

      Attribute_Definition_Source:

          ESRI

      Attribute_Domain_Values:
        Unrepresentable_Domain:
          Sequential unique whole numbers that are automatically generated.
    Attribute:
      Attribute_Label: Value
    Attribute:
      Attribute_Label: Count

Back to Top

Distribution_Information:
  Resource_Description: Downloadable Data
  Distribution_Liability:

      ISU's GIS TReC makes no warranty as to the quality, security, or integrity of this dataset.  Furthermore, users of this dataset assume all responsibility with its viewing, downloading, use, application, and results.

  Standard_Order_Process:
    Digital_Form:
      Digital_Transfer_Information:
        Transfer_Size: 2.201
  Technical_Prerequisites:
    Users must have appropriate GIS and/or remote sensing software to make use of this dataset.

Back to Top

Metadata_Reference_Information:
  Metadata_Date: 20060705
  Metadata_Review_Date: unk
  Metadata_Future_Review_Date: unk
  Metadata_Contact:
    Contact_Information:
      Contact_Organization_Primary:
        Contact_Organization: ISU's GIS TReC
        Contact_Person: Scott Taylor
      Contact_Position: Metadata librarian
      Contact_Address:
        Address_Type: mailing address
        Address:

            Campus Box 8104

        City: Pocatello
        State_or_Province: Idaho
        Postal_Code: 83209-8104
        Country: USA
      Contact_Voice_Telephone: 208 282 3606
      Contact_Facsimile_Telephone: 208 282 5802
      Contact_Electronic_Mail_Address: giscenter@isu.edu
      Hours_of_Service: 9am-4pm
      Contact Instructions:

          When contacting the GIS Center with questions about the preparation and documentation of this metadata file please use e-mail. Include METADATA QUESTION in the subject line and fully identify the document with which you have a question.

  Metadata_Standard_Name: FGDC Content Standards for Digital Geospatial Metadata
  Metadata_Standard_Version: FGDC-STD-001-1998
  Metadata_Time_Convention: local time
  Metadata_Access_Constraints: none
  Metadata_Use_Constraints:
    This metadata document may be used only in ways consistent with the original intent of the document and the GIS dataset that is documents. That is to support geo-spatial analysis, etc.
  Metadata_Security_Information:
    Metadata_Security_Classification_System: none
    Metadata_Security_Classification: Unclassified
    Metadata_Security_Handling_Description:
      n/a
  Metadata_Extensions:
    Online_Linkage: http://www.esri.com/metadata/esriprof80.html
    Profile_Name: ESRI Metadata Profile

Back to Top