# Soils_STATSGO_KFactor.tif

TypeRaster Dataset

TagsNASA RECOVER, GIS TReC at Idaho State University, Wildfire, Western US

### Summary

    This STATSGO-based geologic soil erodibility factor raster image covers the Western US, and was developed specifically to support the NASA RECOVER wildfire decision support system.

### Description

    This STATSGO-based geologic soil erodibility factor raster image covers the Western US and was developed specifically to support the NASA RECOVER wildfire decision support system.

### Credits

    NASA RECOVER, GIS TReC at Idaho State University

### Use limitations

    None, these data were prepared to help support post wildfire decision making.

### Extent

West | -127.839613 | East | -101.342528
North | 51.363111 | South | 29.256654

### Scale Range

Maximum (zoomed in) | 1:5,000
Minimum (zoomed out) | 1:150,000,000

### Topics and Keywords ▼►

Themes or categories of the resourcefarming, environment
Content type ⇔Downloadable Data

Export to FGDC CSDGM XML format as Resource DescriptionNo

### Citation ▼►

Title ⇔Soils_STATSGO_KFactor.tif
Alternate titlesSoils STATSGO Soil Erodibility Factor
Revision date2016-10-28 00:00:00
Presentation formats ⇔digital map

### Citation Contacts ▼►

Responsible party - principal investigator

Individual's nameKeith Weber
Organization's nameGIS Training and Research Center at Idaho State University
Contact's positionGIS Director

### Resource Details ▼►

Dataset languages ⇔English (UNITED STATES)
Dataset character setutf8 - 8 bit UCS Transfer Format
Spatial representation type ⇔grid
Processing environment ⇔Version 6.2 (Build 9200) ; Esri ArcGIS 10.4.1.5686
Credits

      NASA RECOVER, GIS TReC at Idaho State University

ArcGIS item properties

Name ⇔Soils_STATSGO_KFactor.tif
Location ⇔file://C:\Data\RECOVER_metadata\Rasters\Other\Soils_STATSGO_KFactor.tif

Access protocol ⇔Local Area Network

### Extents ▼►

Extent

Geographic extent

Bounding rectangle

Extent type
Extent used for searching
West longitude ⇔-127.839613
East longitude ⇔-101.342528
North latitude ⇔51.363111
South latitude ⇔29.256654
Extent contains the resource ⇔Yes

Extent in the item's coordinate system

West longitude ⇔-2354940.944632
East longitude ⇔-502940.944632
South latitude ⇔992019.949451
North latitude ⇔3165019.949451
Extent contains the resource ⇔Yes

### Resource Points of Contact ▼►

Point of contact - principal investigator

Individual's nameKeith Weber
Organization's nameGIS Training and Research Center at Idaho State University
Contact's positionGIS Director

### Resource Maintenance ▼►

Resource maintenance

Update frequencyannually

### Resource Constraints ▼►

Legal constraints

Limitations of use

      None, these data were prepared to help support post wildfire decision making.

Constraints

Limitations of use

      None, these data were prepared to help support post wildfire decision making.

### Spatial Reference ▼►

ArcGIS coordinate system

Type ⇔Projected
Geographic coordinate reference ⇔GCS_North_American_1983
Projection ⇔USA_Contiguous_Albers_Equal_Area_Conic_USGS_version
Coordinate reference details ⇔

Projected coordinate system

Well-known identifier102039
X origin-16901100
Y origin-6972200
XY scale266467840.99085236
Z origin-100000
Z scale10000
M origin-100000
M scale10000
XY tolerance0.001
Z tolerance0.001
M tolerance0.001
High precisiontrue
Latest well-known identifier102039
Well-known textPROJCS["USA_Contiguous_Albers_Equal_Area_Conic_USGS_version",GEOGCS["GCS_North_American_1983",DATUM["D_North_American_1983",SPHEROID["GRS_1980",6378137.0,298.257222101]],PRIMEM["Greenwich",0.0],UNIT["Degree",0.0174532925199433]],PROJECTION["Albers"],PARAMETER["False_Easting",0.0],PARAMETER["False_Northing",0.0],PARAMETER["Central_Meridian",-96.0],PARAMETER["Standard_Parallel_1",29.5],PARAMETER["Standard_Parallel_2",45.5],PARAMETER["Latitude_Of_Origin",23.0],UNIT["Meter",1.0],AUTHORITY["Esri",102039]]

Reference system identifier

Value ⇔102039
Codespace ⇔Esri
Version ⇔8.1.2

### Spatial Data Properties ▼►

Georectified Grid
▼►

Number of dimensions ⇔2
Axis dimensions properties - column (x-axis)

Dimension size ⇔1852
Resolution ⇔
1000.000000 m (meter)

Axis dimensions properties - row (y-axis)

Dimension size ⇔2173
Resolution ⇔
1000.000000 m (meter)

Cell geometry ⇔area
Point in pixel ⇔center
Transformation parameters are available ⇔Yes
Check points are available ⇔No
Corner points

Point ⇔-2354940.944632 992019.949451
Point ⇔-2354940.944632 3165019.949451
Point ⇔-502940.944632 3165019.949451
Point ⇔-502940.944632 992019.949451

Center point ⇔-1428940.944632 2078519.949451

ArcGIS Raster Properties
▼►

General Information

Pixel depth ⇔32
Compression type ⇔None
Number of bands ⇔1
Raster format ⇔TIFF
Source type ⇔continuous
Pixel type ⇔floating point
No data value ⇔-3.4028231e+038
Has colormap ⇔No
Has pyramids ⇔Yes

### Spatial Data Content ▼►

Image Description

Type of information ⇔image
Attribute described by cell valuesRaster Image
Band information

Description ⇔Band_1
Maximum value ⇔0.640000
Minimum value ⇔0.039000
Number of bits per value ⇔32

Triangulation has been performedNo
Radiometric calibration is availableNo
Camera calibration is availableNo
Film distortion information is availableNo
Lens distortion information is availableYes

### Data Quality ▼►

Scope of quality information
▼►

Resource leveldataset

Data quality report - Conceptual consistency ▼►

Conformance test results

Test passedYes
Result explanation

      Visual review

Product specification
▼►

TitleSoils STATSGO KFactor
Revision date2016-10-31 00:00:00

### Lineage ▼►

Process step
▼►

Description

      Raster pixel containing Soil Erodibility Factor information without data table

### Distribution ▼►

Distribution format

Name ⇔Raster Dataset
Version1.0

### Metadata Details ▼►

Metadata language ⇔English (UNITED STATES)
Metadata character set ⇔utf8 - 8 bit UCS Transfer Format
Metadata identifierAE3AA9C8-3549-4079-8CF4-6DDF8B565E81
Scope of the data described by the metadata ⇔dataset
Scope name ⇔dataset
Last update ⇔2016-11-02
ArcGIS metadata properties

Metadata formatArcGIS 1.0
Metadata styleISO 19139 Metadata Implementation Specification
Standard or profile used to edit metadataISO19139
Created in ArcGIS for the item2016-10-24 16:29:39
Last modified in ArcGIS for the item2016-11-02 16:19:32
Automatic updates

Have been performedYes
Last update2016-11-02 16:19:32

### Metadata Contacts ▼►

Metadata contact - principal investigator

Individual's nameKeith Weber
Organization's nameGIS Training and Research Center at Idaho State University
Contact's positionGIS Director

### Metadata Maintenance ▼►

Maintenance

Update frequencyannually

### Metadata Constraints ▼►

Constraints

Limitations of use

      None, these data were prepared to help support post wildfire decision making.

Legal constraints

Limitations of use

      None, these data were prepared to help support post wildfire decision making.

### Thumbnail and Enclosures ▼►

Thumbnail

Thumbnail type